Crown lift all trees on site by 2-3m.

T1) Re-pollard willow to prevent any further snap outs, remove hanging branch.

T2) Section fell spruce to ground level.

T3) cherry crown lift to 4m and reduce back from path to allow room for tent. 

T4) Fell dead trees.

T5) Thin hazel and crown lift.

T6) Crown lift to 4.5m, reduce top by 2m to form good shape. 

T7) Crown lift over road to 5m. 

T8) Crown lift willow by 4m, pull crown back from building to prevent damage to chimney stack.

T9) Remove hanging branches, crown lift to 4m. 

T10) Remove hanging branches clean up bad pruning points.

T11) Crown lift to 5.5m where overhanging road. 

T12) Fell dead trees to ground level.

T13) Remove shrub blocking fire exit.

T14) Crown lift hornbeam to help better cctv view.

T15) Pull birch back from building remove stem leaning towards building. 

T16) Crown lift to 4m, remove limbs over footpath, reduce weight on large limb over hanging benches. 

G1) Thin out woodland strip so uni buildings are visible from roadside, cut shrubs down to manageable height,
Reduce shrubs back from building, clear road signs and crown lift where over hanging uni roads. 

G2) Pull trees back from building by 1m.

G3) Section fell ash trees with stage 2 ash die back to ground level.

G4) Crown life to fence height. 

G5) Crown lift to 4m and pull back from building by 1m to prevent damage. 

G6) Crown lift to 5m, remove major deadwood and sever ivy.

G7) Crown lift to fence height. 

G8) Crown lift to 4m, reduce end weight on limb overhanging road.

G9) Crown life over road by 5m clean up poor pruning cuts on cherry.

Chip to site when suitable and make tidy, remove chip and timber.
