VAL/2023/0347   Ventilation 

All Bathrooms will require ventilation. 

Due to the low wall  plate height, all bathrooms in both barns will be ventilated via slate vents. 

all slate vents will be positioned in the roof, above the bathrooms. due to the position of the bathrooms in the buildings, no slate vents will be visible from the road. 

the slate vents can be found here https://www.screwfix.com/p/alpha-slate-vent-black/45984?kpid=45984&cm_mmc=Google-_-Datafeed-_-Building%20and%20Doors?kpid=KINASEKPID&cm_mmc=Google-_-TOKEN1-_-TOKEN2&gad_source=1&gclid=Cj0KCQiAo7KqBhDhARIsAKhZ4ugOEUpPp-CHC0OOgwugghlW1cdXdQCPWffBX1V2h28Y45jj6mBlGC0aAg7zEALw_wcB&gclsrc=aw.ds

these are shown in yellow on the overhead image. 

the kitchens will require wall ventilation, these will be terracotta coloured vents situated in the brickwork. again these will not be visible from the roadside. 

these can be found here https://www.cef.co.uk/catalogue/products/1740726-100mm-4-cowled-outlet-with-damper-terracotta?gad_source=1&gclid=Cj0KCQiAo7KqBhDhARIsAKhZ4uhTaAVJxjKVoVeqBHo-R53F-lbI_kc_e00iYgNJK3fTJAXHvICpuhgaAj_OEALw_wcB&gclsrc=aw.ds

these are shown in red on the overhead image

where cavity ventilation is required, as part of the mitigation. terracotta wall vents will be used as per building regulations to allow adequate movement of air between the outer brick wall and inner timber frame studwork.  the wall vents will be approximately 15cm above the outside floor level and will only be installed in barn 2, so these will not be visible from the road.   

the wall vents can be found here https://www.screwfix.com/p/air-brick-terracotta-76mm-x-229mm/13873

please see the overhead image for locations. 

Yellow = slate vents

Red = Wall Vents

Green = Flue pipes 

Kind regards,

Thomas Jones 

