Discharge of Conditions P/2022/0760 + 0761

Condition 4. 

Prior to their use on the building, samples of all new brickwork and pointing shall be submitted to and approved in writing by the Local Planning Authority. 

The bricks will be the ones that we have excavated from the site. they are of the same design as the bricks used in the buildings. therefore will be like for like. 

the mortar mix will be 3:1 measured washed sand and NHL lime. Pointing to be as existing. 

Condition 5.

Prior to their installation on the building, details and locations of all extractors, vents and flues shall be submitted to and approved in writing by the Local Planning Authority. The development shall only be carried out in strict accordance with such details as are approved.

Flue pipes will be black, 5" internal diameter to suit the log burners and rayburn. these will be 4.5 metres high for building regulations. these will not be visible from the roadside as they are at the back of the buildings as per the plans. 

extractors for bathrooms will be terracotta coloured covers where they are visible on the outside wall to help them blend with the colour of the bricks.  again, these will not be visible from the roadside. they will be situated on the outside wall in each bathroom / shower room / kitchen as per the plans. 

Condition 7. 

No further work shall be carried out to any areas of brickwork until details of insulation have been submitted to and approved in writing by the Local Planning Authority. The development shall only be carried out in strict accordance with such details as are approved.

all wall insulation is to be inserted between the internal stud timbers with a breathable membrane stapled to the wall facing side of the studwork with a cavity between the membrane and the external brickwork. 

