Wrexham County Borough Council,

Lambpit Street,

Wrexham

LL11 1AR

RE: P/2022/0760 + 0761  Solution to address concerns in relation to condensation between external and internal walls. 

We have taken advice from our consultant Geraint Roberts regarding reducing the condensation between the external brick and timber wall and the internal stud walls. 

He has suggested digging a drainage trench along the length of the barn. this will be 2400mm away from the external wall on the south side of the barn.  900mm deep with a 150mm perforated pipe bedded on 100mm drainage gravel. this would be deeper than the barn's foundations and would divert the vast majority of rain and ground water around the buildings. therefore reducing the amount of moisture at the buildings foundations. this trench would be covered by the driveways for properties 1 and 2 and would also incorporate the existing drainage plan, making use of the soakaways for the roof gutter water, situated downhill of the properties. 

we will also be removing mortar from one brick perp per panel on property 1 to allow free movement of air in the cavity between the external brickwork and the internal studwork. we have considered using air bricks and plastic weep vents, however we don't think they would be suitable aesthetically, given the oak frame and brick panel design of the building. 

Property 2 will have conventional similarly coloured air bricks fitted to building regulations. 

The top of the cavities on both properties will be open to breath above the wall plate, between the roof rafters. 

