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OPTIMA SCULPTURED CASEMENT WINDOW

Sculptured . Glazing Options
Edge Design 24, 28,36, 40 & 44mm
5 Chamber Sash

(with optional RCM

inserts available) .—Igrll

Outer Frame Sash
10mm Cover on Contro Seals
Weather Seals .ll

6 Chamber Outer
. Frame (with optional

_-- RCM inserts)




