Access Statement

Access to property will be improved by the splaying of walling at 45 deg to enable good visibility both ways

Safety will also be improved for entry and exit to land from entrance without the requirement to open access gate with a measurement to gate from curbline of 5.5m+/- 

Ample off road parking is already available on site with property set back over 9 m from gateway to building line and an estimated 100m2 to RHS of proposed gate position.
