Colin Jones Brunnett Barn, TY Broughton, SY13 3BA  P/2013/0505


Materials proposal for Brunnett and Blossom Barn. 
Brickwork. 
External brick work will be re using existing bricks where required. Lime and sand mix to be used for rebuilding ( where required ) wet lime mix to be used for pointing once all works are completed. Mix to be confirmed by CADW
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Oak framework. 
Most of the external oak framework will remain in place. Any repairs will be done using air dried oak from north Shropshire timber in a traditional style. Any missing timbers will be replaced with air dried oak and will be fitted by using mortice and tennon joints, or splicing. 
[image: ]














Roofing
[image: A picture containing grass, outdoor, ground, stone

Description automatically generated][image: ]Traditional grey 24”x12” and 24”x14” welsh slates and grey pot ridge tiles to be used on the main barn, as per existing roof on adjoining barn. 
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Guttering and downpipes 
A mixture of Aluminium – cast iron style – downpipes and black deepflow upvc half round guttering fixed to the rafter ends and 75mm round downpipes to be used. 
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External windows and doors 
All windows and doors will be constructed of oak and all glass will be doble glazing. 
[image: ][image: ]Doors will be built from oak planks and will look like existing barn doors. Windows will all have pieces of double glazed glass and additional vertical bar to look like a traditional Georgian bar window. 

























Extractors and ventilation.
Brick coloured vent and extractor grilles will be used, mostly at the rear of the buildings- so not to spoil the frontal view of the building. 
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Log burner chimney pipes to be black and traditional.  Fixed to existing brick work. 
[image: twin wall chimney system]
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