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TREE REPORT

Introduction

Canopy Tree Care has been instructed by Fr. Tudor Hughes, to carry out a visual tree assessment (VTA) survey, of the trees at All Saints Church, Gresford. Only those trees within the Churchyard boundaries, as outlined in red were assessed. 
The survey was carried out on 12th March 2022, by Nathaniel Pritchard BSc Cert.Arb.

Nathaniel Pritchard is a fully qualified, certified arborist.  He holds an ABC Level 2 Certificate in arboriculture (Royal Forestry Society), a LANTRA Certificate in Professional Tree Inspection, Bachelor of Science Degree in Biological Sciences, and has had Continued Professional Development over the last 18 years.
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The Survey
The survey aims to determine tree vigour and structural integrity through a non-intrusive visual tree assessment (VTA) from ground level, seeking to ascertain the health and condition of the trees, and any risk they may pose.

The risk posed, refers to the likelihood of a tree shedding branches or falling and causing injury/damage.
When assessing risk, the following factors are considered:

Likelihood of failure – nature of defect and characteristics of tree species.

Impact potential – size/weight of the tree part most likely to fail.

Target object/s – what could be injured or damaged in the event of tree failure.

Probability of striking target – tree failure onto target or failed limb/tree struck by a fast moving target.   
Trees are living entities and are therefore subject to natural processes.  They will also be subject to changes to their environment caused by human’s activities and to exceptional weather conditions.  The inspection undertaken by our qualified staff relies on visual attributes of tree health and structure which can be assessed from a ground based inspection.  Hidden defects which are not readily visible may not be detected.  We therefore cannot wholly guarantee the condition and safety of the trees inspected beyond what can be reasonably assessed from the procedure used.
The findings of the report are limited to the date of the survey. Signs of stress, disease, and decay such as fungi, early or late leaf emergence or leaf fall, size and colour are seasonal and may not have been present at the time of inspection.

Work recommendations have been prioritised based on tree proximity to a target, size and probability of structural failure and potential for future problems to develop as the trees increase in size or as wounds/decay develop with time. 

To establish acceptable levels of safety, it is advised that all tree works be carried out in accordance with the report table recommendations and be carried out within the time scales indicated. 
We recommend that the trees are regularly assessed, and tree surveys carried out every 3 years, with the next assessment to be undertaken on or before March 2025.
Interim inspections are recommended after periods of inclement weather (i.e., storms, gales, etc). Changes in site conditions or usage may also necessitate adjacent trees to be re-evaluated.

Standard of Work
All tree work undertaken should be done in accordance with British Standard 3998:2010 and by competent contractors insured with public liability cover of at least two million pounds.  
Statutory Controls

If the trees on site are subject to any Tree Preservation Orders (TPO’s) or are encompassed within a Conservation Area then statutory permission from the Local Planning Authority (LPA) will be required before any tree works take place.  

Wildlife

All operations should take account of wildlife needs and be planned to take advantage of weather conditions and time of year for minimum damage and disturbance.  If any protected species or nesting birds are present or discovered while the works are taking place all work should cease until contact has been made with Countryside Council for Wales for further advice.  CCW can be contacted on 0845 1306229 or by e-mail to: northernteam@ccw.gov.uk  Specific consideration should be given to the possible presence of roosting bats, which are protected by the Wildlife and Countryside Act 1981 (schedule 5) and included in schedule 2 of the Conservation Regulations 1994.  Ideally, a survey should be carried out to identify any potential roost sites and if bats are found to be present advice should be sought from a person qualified and experienced in handling such matters and fully conversant with the implications of the Act
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Assessor:
N. Pritchard
	Tree No.
	Species
	Age
	Vigour
	Structural Condition
	Stem Diameter

(mm)
	Height

(metres)
	Comments
	Recommendation
	Priority of work
	Re-inspection period

	1
	Yew
	M
	F
	G
	1800
	14
	Ivy on main stem.
	Cut Ivy at base.
	L
	L

	2
	Yew
	Y
	G
	G
	-
	3
	Low multi stemmed tree.
	No action required.
	N
	L

	3
	Cedar
	M
	F
	G
	700
	15
	Small broken branch suspended in crown. Safe at present.
	Remove broken branch. 
	L
	L

	4
	Irish Yew
	SM
	G
	G
	-
	5
	Small tree.
	No action required.
	N
	L

	5
	Yew
	M
	G
	G
	650
	14
	Low branching on main stem encroaching on road. 
	Remove low branches on main stem and crown lift. 
	L
	L

	6
	Yew
	M
	G
	G
	900
	13
	Some low branching. 
	Crown lift to 2m.
	VL
	L

	7
	Yew
	M
	G
	G
	900
	14
	Some low branching.
	Crown lift to 2m. 
	VL
	L

	8
	Yew
	M
	G
	F
	900
	14
	Old wounds and decay in main stem.
	No action required at present.
	N
	L

	9
	Yew
	M
	G
	G
	700
	14
	Low branching.
	Crown lift for access under tree.
	VL
	L

	10
	Yew
	M
	G
	G
	600
	13
	Low branching.
	Crown lift for access under tree.
	VL
	L

	11
	Yew
	M
	F
	G
	1200
	13
	Low branching and Ivy on stem.
	Crown lift for access under tree and cut Ivy at base.
	VL
	L

	12
	Yew
	M
	F
	G
	650
	13
	Low branching. 
	Crown lift for access under tree. 
	VL
	L

	13
	Yew
	M
	F
	G
	600
	13
	Low branching and Ivy on stem. 
	Crown lift for access under tree and cut Ivy at base.
	VL
	L

	14
	Yew
	M
	F
	G
	700
	
	Wide spreading crown and low branching. Ivy on stem.
	Crown lift for access under tree and cut Ivy at base. 
	VL
	L

	15
	Yew
	M
	G
	G
	500 x 2
	15
	Twin stemmed from 0.5m.
	No action required.
	N
	L

	16
	Yew
	M
	G
	G
	400 x 3
	13
	Triple stemmed from 0.5m.
	No action required.
	N
	L

	17
	Yew
	M
	F
	G
	400
	13
	Ivy on main stem.
	Cut Ivy at base.
	L
	L

	18
	Yew
	M
	G
	G
	500
	13
	Ivy on main stem.
	Cut Ivy at base.
	L
	L

	19
	Yew
	M
	G
	G
	700
	13
	Ivy on main stem.
	Cut Ivy at base.
	L
	L
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Assessor:
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	Tree No.
	Species
	Age
	Vigour
	Structural Condition
	Stem Diameter

(mm)
	Height

(metres)
	Comments
	Recommendation
	Priority of work
	Re-inspection period

	20
	Yew
	M
	G
	G
	600
	13
	Low branching towards road.
	Crown lift.
	L
	L

	21
	Yew
	M
	G
	G
	400
	13
	Low branching towards road.
	Crown lift.
	L
	L

	22
	Yew
	M
	G
	G
	900
	13
	Low branching towards road. Ivy on stem.
	Crown lift and cut Ivy at base.
	L
	L

	23
	Yew
	M
	G
	G
	450
	13
	Low branching towards road. Ivy on stem.
	Crown lift and cut Ivy at base.
	L
	L

	24
	Yew
	M
	G
	G
	500
	13
	Low branching towards road. Ivy on stem.
	Crown lift and cut Ivy at base.
	L
	L

	25
	Yew
	M
	G
	G
	600
	13
	Low branching over road.
	Crown lift.
	L
	L

	26
	Cedar
	M
	G
	G
	1100
	22
	Dead and broken branches recently removed. 
Low branches toward road. 
	Crown lift as required.
	L
	L

	27
	Yew
	M
	G
	G
	450
	13
	Low branching.
	Crown lift.
	L
	L

	28
	Box
	M
	G
	G
	250
	6
	Low branching.
	Crown lift as required.
	L
	L

	29
	Yew
	M
	G
	G
	500 x 2
	15
	Twin stemmed from 0.5m. Low branching towards road.
	Crown lift.
	L
	L

	30
	Yew
	M
	G
	G
	300 x 7
	13
	Multi stemmed from near ground level. Low branches over road.
	Crown lift.
	L
	L

	31
	Yew
	V
	F
	F/P
	3000
	14
	Multi stemmed from 1.5m. Significant decay in stem. Reduced recently. 
	No action required at present.
	N
	L

	32
	Yew
	M
	G
	G
	900
	14
	No significant defects. 
	No action required.
	N
	L

	33
	Yew
	M
	G
	G
	900
	14
	Low branching.
	Crown lift to improve access around tree.
	VL
	L

	34
	Yew
	M
	F
	G
	900
	12
	Low branching.
	Crown lift to improve access around tree.
	VL
	L

	35
	Yew
	M
	G
	G
	1000
	13
	Low branching.
	Crown lift to improve access around tree.
	VL
	L
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	Re-inspection period

	36
	Yew
	M
	G
	G
	1000
	13
	Low branching on main stem and Ivy. 
	Crown lift and cut Ivy at base.
	VL
	L

	37
	Yew
	M
	G
	G
	900
	13
	No significant defects.
	No action required.
	N
	L

	38
	Yew
	M
	G
	G
	1000
	13
	No significant defects.
	No action required.
	N
	L

	39
	Yew
	M
	G
	G
	500
	12
	No significant defects.
	No action required.
	N
	L
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Key to Report Tables
Age Class

NE
Newly Established
Easily Transplanted.

Y
Young


Well established and not easily transplanted.

SM
Semi Mature

Still gaining in size, showing strong apical dominance.

EM
Early Mature

Approaching optimum height, apical dominance less distinct.

M
Mature

Reached optimum height for environment.

OM
Over Mature

In natural state of decline.

V
Veteran

Tree that shows features of biological, historical, cultural, 
aesthetic value that are characteristic of individuals surviving 
beyond their typical age range.

Vigour

VG
Very Good

Large leaf size, density. Long extension growth typical in 
young trees.




Tree exceeds expected growth characteristics for species

G
Good


Leaf size, colour, density typical for species.

F
Fair


Smaller than expected leaf size, low leaf density.





Short extension growth typical in mature trees.

P
Poor


Showing signs of stress, sparse crown, small leaf size or loss of 

colour.

VP
Very Poor

Peripheral die-back or signs of significant stress. Tree in 

decline.

D
Dead


Completely dead, showing no signs of life.

Structural Condition

VG
Very Good

Contains no obvious areas of damage or structural defects.

G
Good


Very minor areas of damage or defects not considered 

significant.

F
Fair


Minor areas of damage or defects not significant at present, but 

with the potential to develop as tree grows, or damaged areas 

decay.

P
Poor


Areas of damage or defects that may lead to structural failure.

VP
Very Poor

Contains serious areas of damage or defects.





Structural failure likely.

NB 
Where ‘?’ has been used, measurements/observation cannot be quantified.

This is usually due to visual obstructions such as dense Ivy coverage.
D.B.H

Stem Diameter at Breast Height – measured at 1.3m above ground level.
 

Estimated measurements taken for the purpose of this survey.

Height

Measured in metres from ground level. 
Estimated measurements taken for the purpose of this survey.

Work Priority

U
Urgent


Works required immediately to make tree safe.

VH
Very High

Works required within 30 days.

H
High


Works required within 90 days.

MH
Moderately High
Works required within 6 months.

M
Moderate

Works required within 12 months.

ML
Moderately Low
Works required within 2 years.

L
Low


Works required within 3 years.

VL
Very Low

Works not required as part of Health and Safety Inspection.





(e.g. future tree management, improve aesthetics)

N
None


No works required, no target exists or is excluded.

Re-inspection Period
U
Urgent


Carry out detailed inspection of the areal parts and/or with the 

use of decay detection equipment as soon as can be arranged.

VH
Very High

6 month inspection.

H
High


12 month inspection.

M
Moderate

18 month inspection.

L
Low


3 year inspection.

VL
Very Low

5 year inspection.

N
None


No target exists or is excluded.

Interim Inspections are recommended after periods on inclement weather (storms, gales etc).

Changed in site conditions or usage, may necessitate Inspection Frequencies be re-evaluated.

