P/2018/0684 HENBLAS SQUARE, HENBLAS STREET, WREXHAM
Dust Management Scheme Ref: 2018/001
· The majority of the works will be contained within the building.
· Operations likely to create dust internally, such as the removal of the internal load-bearing walls or the cutting of new door openings, will be managed with local dust suppression measures such as water suppression to Stihl saws. 
· The demolition of the internal staircases will use remote demolition methods which minimise the creation of dust. In this instance, the demolition will be undertaken using a Brokk 90 or similar robotic demolition machine which is quieter, safer, more efficient and produces minimal dust.
· Debris will be removed from the building using a timber lined chute adjacent to the scaffold loading bay in the rear yard. This will be constructed so as to discharge directly into a skip beneath it. All skips will be sheeted before removal from site.  
· There are a small number of new window openings to be formed in the external brickwork walls. All cutting will be performed using water suppression to minimise the creation of dust.
· All core drilling, for services etc., will have water suppression to minimise the release of construction dust. 
· External scaffolding to public highways and pedestrian areas will have debris netting.
· As the work progresses, internal cleaning will be achieved by sweeping with water suppression to remove large debris and by the use of an industrial vacuum cleaner.
· Operatives involved in operations likely to create dust will be face-fit tested and provided with facemasks to FPP3 standard.
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