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VESSEL DELIVERY TO DOMESTIC/COMMERCIAL SITE UPTO 5000 LTR

	METHOD STATEMENT /RISK ASSESSMENT
(The Management of Health & Safety at Work Regulations)

	Client details: 
Site Contact:

Tel:

Account Number:
	
	Main contractor: 

Budget Gas Project Supervisor:

Tel: 

Sub contractor:

Contact:

Tel:
	


	General

Description of work:
	Delivery of LPG storage Vessel(s) onto plinth at customer's premise  

	Objective:


	To provide a Safe System Of Work for the activity.

	Scope:


	Delivery onto plinth of LPG Vessels (above and below ground) up to 5000 Litres water capacity with nominal 100 litres (50kg) LPG content in accordance with LPGA procedures and relevant legislation.

	Reference:


	Control Measures:

Vessel installation and siting

*

                   LPGA Codes Of Practice see opposite
*

*

Use of Crane
	Document  Ref:
LPGA COP 1 : Part 1: Design, Installation and Operation  of Vessels located above Grounds

 LPG Cop 1 Part 2 Bulk LPG Vapour Offtake Small Bulk Propane Installations
*

LPGA COP 20: Automotive LPG Refuelling Facilities

*

*

LPGA COP 26 : Uplifting of LPG vessels & carriage to and from site

Underground vessel installation section

Gas charge vessel movement

Bolting legs to Liquid Offtake Vessels

Delivering Underground Vessels

The Provision of Personal Protective Equipment

*



	Competence & Training:
	The Driver/Crane operator shall have the appropriate Driver license applicable to the gross vehicle weight of the delivery vehicle they are operating.  Compliance with The Carriage of Dangerous Goods by Road Regulations, Class 2 (In tanks).  In addition the person shall have successfully completed training and assessments in the operation of Vehicle Mounted Crane Units (Lorry Loader) appropriate to the equipment they will operate. 

Crane operators may be required to complete a Vessel Delivery Course and assessment depending upon previous experience. 

	Preparation:          1.

2.

3.

4.

5.

6.

                                    7.


	The Budget Project Supervisor or appointed agent shall contact the customer to discuss the delivery process if nessasary with details of the Method Statement and obtain information concerning any site safety rules and control measures that may be required to comply with. (Where applicable amend Method statement to suit).

The Budget Gas Project Supervisor shall select a suitable contractor in accordance with SMS Manual section 5 ensuring that certification confirming acceptance and competance of the contractor is held on file.

The Budget Gas project supervisor or appointed agent shall liase with the crane operator to ensure that the most appropriate lifting tackle is selected to avoid damage to the vessel(s).

Where applicable acknowledge receipt and acceptance of Clients Health & Safety Rules.  

The Budget Gas project supervisor, or appointed agent shall where appropriate carry out a preliminary site inspection to identify any potential hazard(s) at/on the site/in the vicinity of the work area These shall include checks for overhead and underground hazards in the crane operating/standing area.  

The Budget Gas project supervisor, or appointed agent shall discuss any findings with the client's representative and will ensure appropriate control measures are put in place to safe guard persons or property at risk.

The Budget Gas Project Supervisor, or appointed agent shall Liaise with the crane operator and discuss details of the Method Statement, hazards and appropriate control measures and where applicable the Clients Health & Safety rules. 

	Monitoring:           1.

                                2.

                                   3.
	The Budget Gas Project Supervisor or appointed agent shall ensure that the Budget Gas appointed contractor fully complies with the requirements of the Method Statement and where appropriate carry out checks on tools, lifting equipment and PPE.

The contractor shall fully implement the agreed Safe System Of work for the activity as defined in the scope and follow the operation section of the Method Statement and Health & Safety rules.

The contractor shall monitor the agreed Safe System Of Work and liaise with the client's representative as and when appropriate.



	
	· Report to Client, sign in and advise of the work to be undertaken.

· Prior to any lifting operation carry out a site safety inspection to identify any overhead or underground

               hazards.

· Check that there is suitable access and egress for the crane vehicle and can be positioned safely close to the plinth.

· Ascertain that the vessel plinth is suitable for the delivery of the vessel(s) and meets COP 1 requirements.

· Ensure that the vessel siting complies with the requirements of COP 1.

· Ensure there is enough room to operate the crane safely.

· Obtain a Work Permit or permission from the client to proceed with the operation if required.
· Where appropriate position suitable signage to warn others that may be affected by the work or

               Hazards and where appropriate make arrangements for the work area to be cordoned off.

· Prior to lifting the vessel(s) an inspection shall be carried out on the lifting equipment and LPG vessel(s) by a competent person.      

· Where appropriate secure vessel(s) to piers, pre cast anchor blocks in accordance with  

               Work instructions.

· Where appropriate leave additional materials and equipment in a safe and secure place.

· Tidy site and remove any surplus materials.

· Report to client's representative and complete documentation.

· Formally close job; return any permits, passes etc.  


	Hazards:


	Hazard:

· Fire and/or explosion 

· Compressed Gases

· Electrical Shock

· Manual handling activities

· Vehicle movement & operation

· Confined space: -

          - Drowning

 -  Exhaust Gases

 - Collapse of excavation

· Work place, work

         Equipment

· Falling objects

· Physical injury:-

        - cold burns

        - maintenance, fitting etc

        - Slips, trips and falls

        - Cuts and abrasions
	Risk Level:

Low to medium

Low to medium

Low to medium

Low to medium

Low to medium

Low to medium

Low to medium

Low to medium

Low

Low to medium

Low to medium

Low to medium

Low to medium

Low to medium


	Effect:
Injury/property damage

Injury/property damage

injury

injury

injury

injury

injury

injury

injury

injury

injury 

injury

injury

injury

	Personal

Protective

Equipment:
	Hard Hat, goggles, Gloves (for general work and for handling LPG), Overalls, Protective footwear, wet weather protection as required.




	Work Equipment: 1.

2.

                              3.
	Carry out a safety check on all appropriate tools and equipment prior to use.

Untested and poorly maintained tools shall not be permitted. 

Under no circumstances must customer's tools and equipment or services be used unless prior consent is given.  



	Power Tools:


	110v only: Portable hand tools operating at 240v shall not be permitted. 



	Completed by:  Andrew Ashley                            Position:   Health & Safety Coordinator                                                              
Date:  30th December 2014
I confirm that the work shall be completed in accordance with the requirements of the Method Statement.
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