Redevelopment of Caravan Site, Old Wrexham Road, Gresty

DUST CONTROL
SAFETY NOTICE FOR ALL WORKERS

BEFORE YOU START:
1) Make sure you are using equipment that will minimise creation of dust, e.g. cutting machines that have integrated vacuum extraction or water jet.

2) If dust is unavoidable, ensure good supply of ventilation.

3) Make sure you have assessed the risks and have the right training and equipment – if you are unsure, speak to your supervisor

IF YOU HAVE DONE EVERYTHING YOU CAN TO MINIMISE CREATION OF DUST:
4)  Put in place protection measures which protect the workforce as a whole, e.g. screen off work areas, use proper industrial extraction equipment with appropriate filters.

5) Ensure personal protective equipment (PPE) is worn, e.g. dust masks, gloves and goggles. It is essential you are wearing the correct PPE. If you don’t have any PPE, speak to your supervisor or a member of the site management team.

6) If you are involved in cleaning operations, ensure you wear PPE and use a dust suppression spray. If no spray is available, go and get one!

Inhalation of dust can cause breathing difficulties or bring on an asthma attack. Dust can cause eye irritation and, if rubbed in, can cause permanent damage. It can also cause skin rashes so cover up.
These measures are for your well-being and if not followed, you will face immediate disciplinary measures which can include verbal warning, written warning and/or a fine which will be docked at source from your wages.
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