SITE METHOD STATEMENT

Site: Thornleigh Close, Wrexham

Traffic Management

· All deliveries to the site will turn directly into Thornleigh Close and use the turning head at the top of Thornleigh Close, to turn the vehicle before reversing down to the site under supervision, to the designated loading off-loading point.

Site Access Signage

· Bilingual construction site access signage x 2 will be installed either side of the entrance to Thornleigh Drive. (Following advise from Darren Green at Highways Dept)

Site Opening Hours

· Monday - Friday 7.30am til 6.00pm

· Saturday - 8.00 am til 12.00 midday

Site Preparation

· The topsoil will be stripped back and stored to the rear of the site.

· A sub-road will be laid from stone with a hard standing ready for the delivery of the temporary site accommodation and storage.

Site Security

· Security fencing will be set up to the rear of the site. 

· Temporary gates will be added to the new entrance, to the south boundary of the site and the west boundary are already secured by neighbouring properties fencing.

Site Accommodation

· A site office will be on site.

Site Storage

· Covered storage will be in two lockable storage containers 

· Timber store as indicated on plan.

· Bricks to be stored as indicated on plan.

Fuel & Chemical Storage

· A bunded fuel tank will be sited on its own designated fuelling area. 

· There will be a spillage kit on site.

· All contractors will receive induction training and how to respond to an emergency following a spillage.

· All chemicals will be stored in suitable receptacles within the storage container.

Highways Contamination

· There will be wheel wash / jet wash facility on site.

· Should mud be carried onto the estate road - a road sweeper will be made available.

Dust Control

· The creation of dust from cutting / grinding machinery will be suppressed by the usage of water attachments.

· Dust creation on the ground after a long duration of dry weather will be suppressed by the damping down of ground.

Prevention of Water Run Off

· Due to the site sitting in a very shallow depression a sump hole will be dug for the collection of silt. A pump with a float switch to pump clean water into the nearest storm drain located to the front of 22, Bryn Estyn Lane.

Services

· All services are to be installed by the appropriate service providers, who will be responsible for providing method statements for their own machinery / apparatus and insulation of cables, pipes and ducts.

Plant Machinery

· 1 x 10 tonne excavator

· 1 x Bottom neck piling rig and 1 x small 0.5 tonne rig

· 1 x Double compaction roller

· 1 x Vibration compaction wacker

· 1 x cement mixer

· Other small handheld power tools

Toilet and Sanitary Facilities

· To be supplied by a portable temporary toilet and hand washing facility which will be regularly serviced.

