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MEMORANDUM
________________________________________________________________________________

	From:
	Service Manager Environment

	To:


	Head of Community Well-being

and Development


	Our Ref:
	P/2017/0459
	Your Ref:
	P/2017/0459

	Date:
	3 July 2017
	
	


___________________________________________________________________________________

TOWN AND COUNTRY PLANNING ACT 1990

TOWN AND COUNTRY (GENERAL DEVELOPMENT PROCEDURE) ORDER 1995
Location: O. S Grid Ref:  2935 3826 Coal Yard, Lloyds Lane, Chirk
Development:  Outline application for residential development
I refer to your consultation dated 14 June 2017 in respect of the above site

The development site is located on Lloyds Lane, a classified highway subject to a 20mph speed limit for which Welsh Government guidelines recommend a visibility splay of 2.4 x 25m in both directions.

The proposed access provides adequate visibility on to the highway.

The access will be constructed to an adoptable standard with adequate width and kerb radii allowing good manouevrability in and out of the site.  The layout reduces the width of the existing site access and should enhance pedestrian safety for pedestrians. 
The traffic generated by the proposed development will be approximately 6 vehicles in the peak hours and will not therefore have a detrimental impact on the highway.

I recommend that any permission include the following conditions:

CONDITIONS

ZJ11

ACCESS WIDTH

039R

The vehicular access hereby approved shall be a minimum width of 4.8m metres.

ZJ15

VISIBILITY SPLAYS IN BOTH DIRECTIONS (NEARSIDE)

038R
Prior to first use of the development hereby approved the vehicular access shall provide visibility splays of  2.4 metres x 25metres in both directions measured to the nearside edge of the adjoining highway.  Within these splays there shall be no obstruction in excess of 1 metre in height above the level of the nearside edge of the adjoining highway.  The splays shall thereafter be permanently retained clear of any such obstruction to visibility.

ZJ22

PARKING AND MANOEUVRING TO BE KEPT CLEAR

035R
The vehicular parking and turning areas as shown on the approved drawing shall be fully laid out, surfaced and drained prior to first use of the development.  These areas shall thereafter be permanently retained and kept free of any obstruction, and made available solely for the parking and turning of vehicles at all times.

NONSTDC
SUBMISSION OF FURTHER DETAILS 

026R

E06N

E07N
No part of the development shall commence until a scheme detailing the construction of the following has been submitted to and approved in writing by the Local Planning Authority:  

1)
Detailed layout, design, drainage and construction of the proposed site access  

The scheme as is approved shall be fully implemented prior to first use of the development. 

ZJ41

GENERAL LAYOUT

026R
Prior to first use of the development the site shall be laid out in strict accordance with layout plan(s) No. BC -07

ZJ45

CONSTRUCTION TRAFFIC MANAGEMENT PLAN

026R
No part of the development shall commence until a Construction Traffic Management Plan including provisions for contractor parking has been submitted to and approved in writing by the Local Planning Authority and the Plan as is approved has been fully implemented.

ZJ46

NO PRIVATE SURFACE WATER RUN OFF

026R
No private surface water run off shall be permitted to flow from the development site onto the adjoining highway.  An Aco drain or similar shall be provided across the approved access to intercept any such run off prior to first use of the development.

NONSTDC   PRIVATE MANAGEMENT COMPANY

026R

The internal access road and parking areas shall be maintained in perpetuity 


by a Private Management Company.

Service Manager Environment
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