Rowland’s Pharmacy, 3 Chapel Street, Wrexham
AIR CONDITIONING EQUIPMENT 

Design and Access Statement

REASON – air conditioning is required to provide ambient temperature for staff and customers

AMOUNT – 1 no. external condenser serving 2 no. internal recessed cassette units

LAYOUT – located in positions as shown on the plans, on the left elevation of the Pharmacy at high level approx. 2.3 metres from ground level
SCALE – External condenser unit 845mm High x 970mm Wide x 330mm deep.

               - Security cage - 1150mm high x 1150mm wide  x 650mm deep

LANDSCAPING – none – the condenser will be mounted at high level and fixed to the wall of the Pharmacy
APPEARANCE – 

The standard powder coated condensers will be located to the rear elevation of the pharmacy building at high level. The colour of the external condenser and security cage will be powder coated Stukko White – 4.2Y/7.5/1.1.

ACCESS – The unit does not obstruct access or egress to the pharmacy. Access to the unit will be just for maintenance via the pathway. Access to the pathway will not be affected by the unit as it at high level  
Noise Impact Statement

The noise impact of the unit is minimal. The sound output is 49dB at 1 metre which is equivalent to “A quiet Library and an average Home” according to the table of Sound Levels attached to the application. The sound level reduces by 6 dB per doubling of distance.
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