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Demolition of low Level Structures
Details of the Project

The works comprise of low level demolition to two sections of a nursing home to make way for a new double storey wing. There is demolition to take place and the construction of a new carpark.

Location

Chirk Court ids located off Chapel Lane B5070.Access will be via the existing road to the nursing home until the new opening off Chapel Lane is constructed.

The site in General

The site is currently in daily use and is an operational residential home. Elderly people are living on site and there are frequent visitors to site.

Dust Mitigation Plan

Dust emissions must be avoided at all costs and extreme care and caution will be taken when planning the work and more importantly when undertaking the work.

All works will be planned with the prime aim of reducing  dust generation.

Where techniques can be adopted to reduce or eliminate potential for dust generation then they will be incorporated into the works.

The site will be constantly monitored by the site supervisor for dust and works will cease immediately should any dust which cannot be controlled is emitted.

Vehicles will be restricted to 10 MPH when on site and there will be no undue over revving of engines to avoid generation of dust.

Haul roads will be wetted down using fine water mists if they appear to be drying out.
Surrounding public roads will be kept clean using lorry mounted sweepers as and when required.

Engines of machines will be shut down when not in use to avoid emitting excessive exhaust fumes

All machines will be serviced in accordance with current manufacturer’s recommendations and exhaust systems checked to ensure a clean burn of exhaust particulates therefore reducing fumes and obnoxious gases to the atmosphere.

Demolition will be undertaken in a controlled manner thus avoiding any sudden collapse which could potentially generate dust.
Demolition works will be undertaken using an excavator which will be attached with a demolition grab which will grip and get hold of part of the structures easing them to the ground.

Soft strip of the building will take place whist all external walls are in situ to avoid any dust release

Windows and external doors will be removed as a last operation prior to the final demolition to contain all work activities.

All vehicles entering and leaving site will be sheeted

All skips will be sheeted prior to leaving site and all will be supplied with high sides to avoid windblown nuisance.

Lidded skips will be supplied for light materials such as the polystyrene insulation material.

All polystyrene will be hoovered up and bagged before being placed in secure containers

All rubbish and waste will be placed directly in skips and will not be left lying loose around the site.

The site will be kept clean and tidy 

All operators will undergo regular tool box talks which will explain and reiterate the importance of eliminating dust generation on site. 

Hydraulic hammers will be serviced and when in operation will be subject to water sprays continually damping down at the point of impact between the chisel and concrete.
During excavation and removal of the concrete water mists will be used to supress any dust.

The loading excavator will carefully load the offsite vehicles ensuring the concrete is placed carefully into the tipper body. The load will not be dropped from height.
Vehicles will not be overloaded thus avoiding debris falling from the vehicle when they are leaving site

Water hoses will be trained on the point of contact between the machine and building and a fine water spray will be fired at the work area to suppress any dust.

Concrete floor slabs will be wetted down with water hoses
Works will stop if the dust cannot be contained and alternative methods of work formulated.

Wind speed and direction will be monitored and should wind speed s become excessive then suspension of certain parts of the works will be considered.
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