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Gas Mitigation Statement

	Building Control Ref Number
	BA/1314/0149

	Associated Planning Ref Number 
	P/2012/0875

	Developers Name
	Ventura Developments

	Site Address
	Land @ St Paul’s, King Street, Cefn.

	Plot Numbers Inspected
	Plots 5 & 6

	Date Inspection Completed
	3rd April & 11th June 2014


Documents associated with Gas Precaution Measures
( Ashton Bennett Consultancy Site Investigation – November 2007
( Strata Site Surveys – Ground Investigation – November 2012
( Building Control Application drawings, specifications & manufacturers details.

( Building Control Application inspections & Notes

Gas Precaution Measures Inspected

Building Regulation Compliance on this site was undertaken by The Building Control Service of Wrexham County Borough Council. 
The inspection regime consisted of 2 inspections of the 2000G Gas Barrier Membranes in situ which were installed in accordance with the manufacturers recommendations and BBA
12/4898 certification. 

The inspections undertaken identified the correct gas membrane product, the condition of the membrane after installation, joining and overlapping including taping details, top hat & corner details and sealing of the cavities. All photograph’s show satisfactory installation of the above.

The membranes are fitted over a beam & pot concrete floor system which is fully ventilated in the void immediately below the structure.

I have attached our inspection regime including the surveyors notes following the inspections.

I hope this report is sufficient for you to consider any planning conditions that require approval for the site.

Surveyor notes following inspection of Gas Membrane Plot 5 & 6.
	25/09/13

8/11/13

	DRM

DRM

	05 – S

04 - S

	On site with agent & ground workers. 1200 gauge dpm being provided over 100mm Quintherm floor insulation (with 25mm around perimeter) over gas membrane suitably lapped and sealed around service penetrations over suspended floor. See photographs. Ok to place concrete. Next inspection – cavity tray dpc.

On site with bricklayers. Cavity tray / weepholes satisfactory.



Photographic Evidence

Plots 5 & 6 King Street, Acrefair.
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