Wrexham CBC Local Planning Authority P/2022/0650
HRA Screening Report for Phosphate inputs in the river Special Areas of Conservation (SACs)

	River Dee and Bala Lake/ Afon Dyfrdwy a Llyn Tegid (UK0030252)

	Annex I habitats present which are a primary reason for selection of this site: 
	· 3260 Water courses of plain to montane levels with the Ranunculion fluitantis and Callitricho-Batrachion vegetation 



	The Annex II species that are a primary reason for selection of this site are: 

	· 1106 Atlantic salmon Salmo salar 

· 1831 Floating water-plantain Luronium natans

	Annex II species present as a qualifying feature, but not a primary reason for site selection: 
	· 1095 Sea lamprey Petromyzon marinus 

· 1096 Brook lamprey Lampetra planeri 

· 1099 River lamprey Lampetra fluviatilis 

· 1163 Bullhead Cottus gobio 

· 1355 Otter Lutra lutra



SCREENING FOR PHOSPHATE INPUTS

	Planning reference:


	P/2022/0650

	Site Name:


	 FORMER METHODIST CHAPEL PONT Y BLEW CHIRK WREXHAM   LL14 5BH

	Description of development:


	TRAWSNEWID ADEILAD I ANNEDD / CONVERSION OF BUILDING TO DWELLING


	SAC River catchment 
	River Dee



	Phosphate inputs: NRW have advised that the following types of development are unlikely to increase phosphate inputs:

	
	Type of development - NRW criteria:
	Relevant information:
	Comments / observations:
	Criterion satisfied: 

	1.
	Any development that does not increase the volume or concentration of wastewater;
	
	
	N/A

	2.
	Any development which improves existing water quality discharges by reducing the phosphate load of wastewater, or by decreasing the volume of wastewater produced (e.g. by improvements to existing wastewater treatment infrastructure);
	
	
	N/A

	3.
	Any development connecting to a public wastewater treatment works where the permit has phosphate conditions in place and the sewerage undertaker has confirmed that there is capacity to treat the additional wastewater and the additional phosphate from the proposed development;
	
	
	N/A

	4.
	Private sewage treatment systems discharging domestic wastewater to ground into drainage fields constructed to the relevant British Standards and which are located more than 50m from the SAC (or a hydrological pathway to the SAC), and which have a daily discharge rate of less than 2 cubic metres (m³)
	Application Form; Submitted Plans; Submitted Supporting Information/Docs.
	New treatment plant would discharge directly to nearby watercourse, and therefore fails to comply with the screening criteria.
	No

	5.
	Development to an existing residential property (e.g. extensions) that does not increase occupancy or the volume of drainage.
	
	
	No

	

	Wrexham CBC concludes that:
	A full HRA Screening and Appropriate Assessment will be undertaken in consultation with Natural Resources Wales.

	Where increases in phosphate inputs in the SAC can be ruled out as a result of this development, the following wording is to be read in conjunction with the Officer’s report:
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