Design and Access Statement for replacement windows in a conservation area


Replacement to be made at 43 Ruabon Road Wrexham LL13 7PL










Application Outline

· This application is for replacement of the current front windows at 43 Ruabon Road which is a detached property built in the early Victorian period.

· The property is within the conservation area and not listed.

· The proposal is to replace all the windows shown on the front elevation with casement windows. The windows will be painted in the same colour.

· The windows are the same dimensions as the windows they’re replacing.

· The design specification for all windows has already been supplied

· The current windows were replaced in the early 1980s, are single glazed with timber frames.

· The frames have been repaired a number of times with wood filler and are now in very poor condition with some windows cracked. 

· [bookmark: _GoBack]Being in the conservation area, planning has insisted on timber frames as this would be in keeping with the property and the conservation area.

· The replacement windows have been designed to match the style of the existing windows. 
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Property for which planning permission has been sought shown in red. Access can be gained via the side of the property which has its own driveway.






Front Elevation
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View of front of property from Ruabon Road
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Left side bay window
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Right side bay window














[image: ]Right side upper window
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Left side upper window








[image: ]Middle upper window


















[image: ]Current state of windows Cracked window



[image: ]Rotten window frame


[image: ]Mould on internal walls below window








[image: ]Mould on blind in spite of constant cleaning







· Front openers no longer open leading to moisture in the air becoming trapped and mould developing on walls.

· In the winter the dehumidiyer is on 24 hours a day and has recorded a moisture level of 80% in the living room.

· Rotten frames let in moisture when it rains and this, together with condensation has led to a great deal of mould around the blinds and on the wall under the window. 

· The existing single glazed windows have a poor thermal performance. Double glazed windows will be much more energy efficient and help reduce gas used for heating the property

· Replacement of existing windows will enhance the overall look of the property and improve environmental impact.
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