DRAFT

[image: image2.jpg]W
wrexham
COUNCIL
CYNGOR

wrecSdim




MEMORANDUM
________________________________________________________________________________

	From:
	Chief Officer, Environment & Technical


	To:

FAO:
	Chief Officer Planning & Regulatory 

Sarah Hill


	Our Ref:
	ET/DC/MM/P/2022/0740
	Your Ref:


	P/2022/0740

	Date:
	11th November 2022
	
	


___________________________________________________________________________________

Sycamore House, Wrexham Road, Holt, Wrexham LL13 9YU
Reconstruction of sandstone wall and creation of splayed entrance, alterations to driveway and erection of dividing wall

Further to your email / consultation dated 09/09/2021 in respect of the above, I comment as follows: -
The application includes the alteration of the existing access to the property and the construction of a car port. 
Access

The existing access has inadequate visibility due to the boundary wall. The proposed splayed entrance increases the width of the access from 4.2m to 12m at the kerb. Although the visibility splays appear to fall short of the 2.4 x 43m splays usually required on a 30mph road, the proposed design significantly increases visibility in both directions. 

The replacement gate is to be set back from the road, allowing for vehicles to stop off the highway while the gate is opened and closed. 

Site Layout and Parking
The proposed design allows sufficient space for vehicles to turn on site, allowing them to enter and exit the site in a forwards gear. 
The provision of a car port for six vehicles is in excess of the maximum four spaces that would be permitted by the Wrexham County Borough Council Parking Standards for a new development, but appears to formalize rather than increase the existing parking provision at the property. 

Conclusion 

The proposed design offers a significant improvement to the existing access arrangements. I therefore support the proposal. It is recommended to condition that the access be set out as on the submitted design, ensuring that the visibility splays provided are not less than those shown.
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Chief Officer, Environment & Technical
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