DESIGN AND ACCESS STATEMENT

The proposal is to insert two small (2ft x 3ft) wood framed windows into the existing alcoves either side of the fireplace,
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These windows will match in style and size the existing window (outlined in red on the picture) on the first-floor East elevation. 
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Description automatically generated with medium confidence]However we would copy the header and footer brick detail of the windows on the front (East facing) elevation.
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