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Product Details

RS Pro IP65 Floodlight

This RS Pro 300W LED Floodlight has an ultra slim line body for an aesthetically pleasing look and discrete installation. With a small form factor and it being extremely light, this makes for an effortless install. Also this floodlight is built around an IP65 protection rating so makes ideal use for indoor or outdoor use.

Features and benefits:
• Highly efficient LEDs means less power consumption
• Long life span of up to 30,000 hours
• 27,000 lumen output for remarkable brightness
• Cool white light for brightness and improved concentration
• IP65 rating allows you to use this outdoor too. Dust proof and will deflect water spray from any angle.
• 220-240V AC
• Lumen efficiency of 90lm/W
• Built from quality aluminium and toughened glass for a prolonged life




Specifications

	Attribute
	Value

	Wattage
	300 W

	Voltage
	220 → 240 V ac

	IP Rating
	IP65

	Luminosity
	27000 lm

	Dimensions
	428.6 x 70 x 470.6 mm

	Colour Temperature
	4000K

	Height
	470.6mm

	Life Hours
	30000h

	Width
	428.6 mm

	Depth
	70 mm

	Range
	REX Slim

	Lamp Type
	LED

	Beam Angle
	115°

	Floodlight Type
	Outdoor


