
Starbucks Building:

Roof Sheets 
Profile - Kingspan Topdek – Membrane Armour Plan Quadcore - Light Grey
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Feature Cladding
Bennets Timber BEN-STAR1 Profile in Larch. 125mm cover width finished in Teknos Paint System Base Coat: Wicker and Top Coat: Cypress
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Feature Cladding
Eternet Equitone Facade Panels – Linea LT60
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STARBUCKS EMEA STORE DESIGN - 2020




