Redevelopment of Caravan Site, Old Wrexham Road, Gresty

DUST MANAGEMENT PLAN

Introduction:
The existing caravan site is to be cleared to provide a development site for new housing.

Impact on air quality during construction:
The following aspects have been identified which could directly affect the quality of air in the immediate environment:
1) Dust creation from demolition of the existing structures
2) Dust creation from waste skips
3) Dust creation from breaking up of existing concrete hard standings and crushing to create hardcore for the new development
4) Dust creation from cutting of masonry, timber and associated materials
5) Dust creation form movement of plant around the site

Precautions:
The contractor/client partnership is committed to environmentally sound policies and working practice and offers the following for consideration:
1) Off-site fabrication will be maximised and on-site cutting minimised. Where unavoidable, dust suppression systems will be used on all cutting operations.

2) The use of skips will be minimised and where unavoidable will be damped down prior to collection and will have dust covers fitted as a matter of course.

3) All mechanical plant will have exhaust filters fitted and generally run off low emission fuels, such as two-stroke or diesel. Cutting discs will be fitted with water-fed suppression systems.

4) Deliveries to site will be planned so as to minimise the number of separate deliveries thereby cutting down on generation of dust associated with vehicle turning etc.

5) During demolition, a water spray will be available at all times to control dust.

6) During breaking up of slabs, the crusher plant will be have an integrated water-fed suppression system.

7) Access routes within the site will be constructed along the lines of the internal highway system at an early stage so as to minimise the risk of dust creation from simple “packed earth” roads. In dry conditions, these will be hosed down to prevent air-borne dust.

Monitoring:
Throughout the construction process, the site manager will ensure all precautions are in place and operatives are fully informed through tool box talks; a stand-alone document on dust control forms part of the site rules. If any operatives or subcontractors feel further controls are required, the site rules provide for a health and safety forum during which they can bring their concerns to the site manager. Similarly, the site manager can report directly to the client if he feels additional measures are required.
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