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15th August 2017
Percolation Test

Re:-  Porosity tests on land at station House, Old Road, Minera, Wrexham
Test Results No1
Date:-  14th August 2017
Weather conditions:-  Dry and overcast 
Excavation:-  Holes excavated using JCB.

Location of trial holes:-  proposed site.

Ground conditions:-  Ground consisted of 600mm rubble fill (average depth), 400mm (average depth) ballast/ash.  Ballast/Ash level continued beyond bottom of trial holes.

Trial holes excavated 300mm square and 300mm deep as stipulated in Approved Documents Part H 2010

Trial Hole


No.1


No.2


No.3
Initial Depth (mm) 75%
225mm

225mm

225mm

Final Depth (mm) 25%
75mm


75mm


75mm

Initial Time (sec)

   0


   0


   0

Final Time (sec)

921


988


1027
Average Time 


6.14


6.59


6.85
to fall 1mm (sec)

Percolation Value (Vp)
6.14


6.59


6.85
Average Percolation Value (Vp)
=
6.53 sec/mm   (0.5513 m/hr)
