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Condition 13

The details required by condition 01 shall include details of the location and layout of vehicular parking, turning facilities and loading/unloading areas and a timetable for the provision of the parking, turning and unloading areas. Vehicular parking, turning and loading areas shall be laid out, surfaced and drained in strict accordance with the details as approved and thereafter permanently retained and kept free of any obstruction, and made available solely for the parking, turning, loading and unloading of vehicles at all times.


Response :

Drawings included providing information to discharge condition 13:

· Site masterplan – NWP-AR-CAP-099-PA-01-1001 rev P07
· Site Wide Tracking 16.5m Articulated Vehicle – NWP-CE-TPS-099-DR-XX-021 rev P02
· Site Wide Tracking 12m Rigid Vehicle – NWP-CE-TPS-099-DR-XX-022 rev P02
· Site Wide Tracking 10.7m Articulated Vehicle – NWP-CE-TPS-099-DR-XX-023 rev P02
· Site Wide Tracking 8m Box Van – NWP-CE-TPS-099-DR-XX-024 rev P02
· Support Building Tracking – NWP-CE-TPS-099-DR-XX-025 rev P02
· Access road details – NWP-CE-TPS-099-DR-XX-5001 rev P01
· Vehicle Entry /. Exit Routes – NWP-CE-TPS-099-DR-XX-5004 rev P02

The above information confirms the following :

· Site layout indicates where staff, visitors and service vehicles will enter and leave the site. 
· Clarifies that the parking area is located to avoid the land that is to be maintained as a habitat mitigation area.

We also confirm the following :

· The parking as drawn complies with LPGN 16 i.e. 2400mm x 4800mm for standard parking bays and 3600mm x 4800mm for disabled parking bays, with 6000mm wide aisles between parking bays.
· That all Car Park and Service Area surfacing will be complete prior to first occupation

For information, the zone currently shown on the site masterplan as “Expansion Car Park” would if developed allow for a further 100 cars to park on site.  This car parking zone will only be developed if the current provision of 422 spaces is found over time to be insufficient.  Prior to this being developed Wrexham CBC will be consulted and agreement to the expansion approved by Wrexham CBC.



Documentation Provided :
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