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Flat pent roof covered with a high quality EPDM rubber roof covering.  
Down flow pipe fitted to drain off excess water.
Appropriate guttering to be installed to flow into a water butt with the water to be recycled and used for watering the garden through the year.
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