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Project: Hydro Aluminium Site Redevelopment, Wrexham Industrial Estate 
Date: [Insert Date] 
Delivered By: [Insert Site Manager Name]
1. Introduction
With current works underway, the creation of nuisance dust and silica dust is inevitable due to the nature of the muck away operation, movement of vehicles and preparation of the site for the next phases of the project. 
If we don't manage the dust, we aren't just risking complaints from the neighbouring businesses here on the industrial estate—we are risking our own lungs.
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2. The Hidden Danger: Silica Dust (RCS)
General site dust from dry earth is a nuisance, but silica dust is a killer. Silica is a natural mineral found in concrete, bricks, mortar, and paving.
· When we cut, drill, or grind these materials, it creates fine, invisible dust called Respirable Crystalline Silica (RCS).
· Breathing this in acts like tiny blades in your lungs. Over time, it causes Silicosis (scarring of the lungs), COPD, and lung cancer.
· The rule is simple: If you are cutting concrete or blocks, you must use equipment with on-tool water suppression. No dry cutting on this site.
3. Our Site Rules for Dust Control
To protect ourselves, the local community, and stay compliant with our environmental plan, here is what we are doing:
· Damping Down: We will use water sprays during dry and windy conditions, especially while the excavators are doing earthworks. If your work area is getting too dusty, stop and ask for the water bowser.
· Speed Limits: The site speed limit is strictly 10mph. Driving faster kicks up unnecessary dust. Keep your speed down.
· Keep it Covered: All skips and lorries carrying loose muck or materials must be covered before moving.
· Wear your PPE: Appropriate PPE, including correctly fitted FFP3 dust masks when doing high-risk tasks, must be worn at all times.
4. Your Responsibilities
· Check your gear: Make sure your water suppression bottles are full and working before you start cutting.
· Speak up: If you see a dust cloud forming from an excavation or a dumper run, report it so we can get it damped down.
· Respect the neighbours: We are in an established industrial zone. Dust blowing off-site causes complaints and can get the site shut down by Wrexham Council.


Toolbox Talk Sign-Off Sheet
By signing below, I confirm that I have attended this toolbox talk, understand the dangers of site dust and silica, and agree to follow the site rules for dust management.
	Print Name
	Signature
	Trade / Role
	Date
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